(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(41 "Cmts.User" user "User.Comments")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 145.9375 114.05)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gbr")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VCC")
	(net 3 "TX-SWC")
	(net 4 "SDA")
	(net 5 "SCL")
	(net 6 "RX-SWD")
	(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
	(net 8 "unconnected-(U1-PB7-PadD3)")
	(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
	(net 10 "nRST")
	(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 159.0625 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J53"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 167.1275 144.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP15"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**42"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 157.2775 132.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 140.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J54"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**121"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**65"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 157.1275 144.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP14"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**93"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**83"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**179"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**91"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**3"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 117.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J16"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**164"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 152.8125 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J55"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**49"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**113"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 175.328 114.5065 90)
		(property "Reference" "U4"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**40"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**85"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**46"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 120.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J18"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**154"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**125"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**57"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**122"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**34"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**153"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 175.328 134.5065 90)
		(property "Reference" "U12"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**155"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 147.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J60"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**123"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**115"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 165.328 144.5065 90)
		(property "Reference" "U15"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 149.0625 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J49"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**9"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**87"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**71"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**89"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**86"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 179.0625 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J45"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**14"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**70"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 120.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J22"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**53"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 167.2775 132.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 147.2775 122.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**50"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**74"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 157.2775 112.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 147.1275 124.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP5"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**143"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**24"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**36"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**151"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**10"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**26"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**99"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 169.0625 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J41"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 146.6535 113.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**90"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**166"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 149.0625 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J17"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**130"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 147.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J64"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**35"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 145.328 114.5065 90)
		(property "Reference" "U1"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WLCSP12_1P7X1P42_STM")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**159"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 162.8125 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J43"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 140.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J50"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 176.6535 123.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**59"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**175"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**60"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**39"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**134"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 177.1275 144.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP16"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**147"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**79"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**58"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 159.0625 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J5"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**38"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 145.328 124.5065 90)
		(property "Reference" "U5"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**76"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**144"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**78"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**106"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**84"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**82"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**119"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 179.0625 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J13"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 167.1275 114.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP3"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 157.2775 122.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 172.8125 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J63"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 142.8125 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J19"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 167.1275 134.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP11"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 176.6535 113.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**136"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**100"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**92"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 142.8125 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J35"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**68"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 145.328 134.5065 90)
		(property "Reference" "U9"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**47"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**177"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**161"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**124"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**13"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**120"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**1"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 169.0625 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J57"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 159.0625 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J37"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**116"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**140"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 175.328 144.5065 90)
		(property "Reference" "U16"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**107"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 149.0625 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J33"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 117.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J12"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 130.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J42"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**62"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 140.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J58"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**176"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**2"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**98"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 157.1275 114.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP2"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**31"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**55"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**162"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**156"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 137.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J36"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**133"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 166.6535 133.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 155.328 114.5065 90)
		(property "Reference" "U2"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 137.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J40"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**101"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**73"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**11"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 149.0625 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J1"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 117.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J8"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 127.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J24"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 110.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J2"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 177.2775 112.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**6"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**7"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 152.8125 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J7"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**158"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**126"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**17"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**8"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 147.2775 112.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**72"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**54"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 117.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J4"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 137.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J44"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**16"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 145.328 144.5065 90)
		(property "Reference" "U13"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 162.8125 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J27"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 167.2775 122.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 165.328 114.5065 90)
		(property "Reference" "U3"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 120.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J26"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 110.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J6"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 175.328 124.5065 90)
		(property "Reference" "U8"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 172.8125 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J31"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**69"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**29"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**103"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 177.1275 124.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP8"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 169.0625 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J25"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**167"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**118"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 147.1275 134.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP9"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 179.0625 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J29"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 166.6535 113.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**75"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**45"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 147.2775 142.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 110.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J10"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**41"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**110"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 130.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J46"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**95"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**114"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 167.8375 127.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J28"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 157.1275 124.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP6"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 146.6535 143.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**137"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 156.6535 113.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**27"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**37"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**171"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 166.6535 123.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**80"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**141"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**127"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**138"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 177.1275 114.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP4"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 165.328 134.5065 90)
		(property "Reference" "U11"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**180"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**109"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 172.8125 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J15"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**77"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 165.9375 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**23"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**52"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 155.328 134.5065 90)
		(property "Reference" "U10"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 125.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**64"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**67"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**131"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 146.6535 123.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 156.6535 133.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 145.9375 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.9375 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**146"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**30"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**66"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 176.6535 133.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 162.8125 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J59"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**148"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 152.8125 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J23"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 147.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J52"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 124.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**43"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**4"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 152.8125 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J39"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**172"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 167.2775 112.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**20"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 142.8125 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J3"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**129"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 147.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J56"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**139"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**61"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**22"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**152"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**44"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**128"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 142.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**165"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 165.328 124.5065 90)
		(property "Reference" "U7"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 134.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**102"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 167.2775 142.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 127.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J32"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 156.6535 143.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 146.6535 133.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 110.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J14"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**28"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**174"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 172.8125 135.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J47"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 167.1275 124.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP7"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**21"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 177.2775 122.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 155.328 144.5065 90)
		(property "Reference" "U14"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 157.2775 142.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 157.8375 130.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J38"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 147.1275 114.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP1"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "stm32.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**33"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**108"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**150"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 147.2775 132.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 156.6535 123.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 130.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J34"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 177.2775 132.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**51"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**25"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**173"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 179.0625 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J61"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 180.6975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**81"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 140.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J62"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 169.0625 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J9"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**112"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**135"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 147.1275 144.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP13"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 176.6535 143.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**160"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**5"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 147.8375 127.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J20"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**145"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 154.6675 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**97"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 157.2075 109.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**12"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 177.1275 134.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP12"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**94"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 144.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**163"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 161.1975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**18"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**104"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 162.8125 115.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J11"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 164.6675 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**157"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 150.6975 115.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 157.1275 134.52)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP10"
			(at 0 -1.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm"
			(at -0.1 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0.3 -3.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 10 "nRST")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 128.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**63"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 119.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**48"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 159.0625 125.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J21"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TX-SWC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 138.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**111"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 137.175 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J48"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RX-SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 147.2075 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**96"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**117"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**168"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "CBA / Fab lib:STM32C011D6Y6TR"
		(layer "F.Cu")
		(at 155.328 124.5065 90)
		(property "Reference" "U6"
			(at 0 1.75 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STM32C011D6Y6TR"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "CBA / Fab lib:STM32C011D6Y6TR"
			(at 0.5 -4 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3 -0.6 -90)
			(layer "F.Fab")
		)
		(pad "A2" smd circle
			(at -0.1515 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at 0.4545 -0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(U1-PC15-OSCX_OUT-PadA4)")
			(pinfunction "PC15-OSCX_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1" smd circle
			(at -0.4545 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RX-SWD")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at 0.1515 -0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SDA")
			(pinfunction "PC14-OSCX_IN")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -0.1515 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA14-BOOT0")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at 0.4545 -0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VCC")
			(pinfunction "VDD/VDDA")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -0.4545 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(U1-PA11PA9{slash}PA8-PadD1)")
			(pinfunction "PA11PA9/PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D3" smd circle
			(at 0.1515 0.0875 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(U1-PB7-PadD3)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "E2" smd circle
			(at -0.1515 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "TX-SWC")
			(pinfunction "PA12PA10/PA7")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at 0.4545 0.2625 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS/VSSA")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -0.4545 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(U1-PA3{slash}PA4{slash}PA5{slash}PA6-PadF1)")
			(pinfunction "PA3/PA4/PA5/PA6")
			(pintype "bidirectional+no_connect")
		)
		(pad "F3" smd circle
			(at 0.1515 0.4375 90)
			(size 0.2032 0.2032)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "nRST")
			(pinfunction "PF2-NRST/PA0/PA1/PA2")
			(pintype "bidirectional")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**178"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 174.6675 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**169"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 144.6675 139.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**142"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 177.2775 142.56 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0.742462 -0.13435 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "detail" "16V, X5R, +/-10% (4.7uF also OK)"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.72832 0.021213 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 145.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**149"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 175.9375 148.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**170"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 177.8375 120.925 -90)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J30"
			(at 0 -1.695 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 270)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 167.2075 118.79 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**15"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 160.6975 132.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**105"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 151.1975 122.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**56"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 166.6535 143.165 -45)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.05 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 nF"
			(at -0.87752 0.007778 -135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0201_0603Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "details" "16V, X7R, +/-10%"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.861963 -0.006364 -135)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 315)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "dm_connector:socket_1x04_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 142.8125 145.95 180)
		(descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.27mm single row")
		(property "Reference" "J51"
			(at 0 -1.695 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 5.505 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "dm_connector:socket_1x04_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.905 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1.55 1)
			(drill oval 1.25 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 177.2075 129.29 90)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**132"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 141.1975 135.32)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**88"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 171.1975 112.78)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**32"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 170.6975 114.05)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**19"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Hole_0.5mm"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0.2286 5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "F&B.Cu")
		)
	)
	(footprint "dm_connector:dm_qr"
		(layer "B.Cu")
		(at 145.9375 114.05 180)
		(property "Reference" "G***"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "dm_connector:dm_qr"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_line
		(start 163.4375 138.8)
		(end 164.4175 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 131.55)
		(end 170.6875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 138.8)
		(end 168.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 138.8)
		(end 148.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 135.57)
		(end 151.1875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 139.3)
		(end 158.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 109.3)
		(end 178.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 119.3)
		(end 171.1875 121.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 135.57)
		(end 160.6875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 129.3)
		(end 164.4175 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 141.55)
		(end 151.1875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 115.57)
		(end 150.6875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 128.8)
		(end 158.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 109.3)
		(end 168.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 145.57)
		(end 151.1875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 115.57)
		(end 161.1875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 131.55)
		(end 171.1875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 146.55)
		(end 178.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 139.3)
		(end 161.1875 141.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 131.55)
		(end 178.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 118.8)
		(end 144.4175 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 148.8)
		(end 168.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 138.8)
		(end 178.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 118.8)
		(end 178.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 128.8)
		(end 174.4175 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 139.3)
		(end 164.4175 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 145.57)
		(end 180.6875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 136.55)
		(end 143.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 109.3)
		(end 154.4175 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 119.3)
		(end 148.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 131.55)
		(end 150.6875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 135.57)
		(end 170.6875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 125.57)
		(end 171.1875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 115.57)
		(end 141.1875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 128.8)
		(end 144.4175 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 136.55)
		(end 168.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 128.8)
		(end 148.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 116.55)
		(end 148.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 146.55)
		(end 173.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 148.8)
		(end 174.4175 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 129.3)
		(end 168.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 125.57)
		(end 160.6875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 139.3)
		(end 151.1875 141.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 121.55)
		(end 158.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 129.3)
		(end 141.1875 131.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 111.55)
		(end 141.1875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 125.57)
		(end 170.6875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 126.55)
		(end 178.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 126.55)
		(end 143.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 135.57)
		(end 161.1875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 116.55)
		(end 178.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 146.55)
		(end 143.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 131.55)
		(end 158.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 136.55)
		(end 173.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 139.3)
		(end 168.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 138.8)
		(end 144.4175 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 141.55)
		(end 148.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 121.55)
		(end 148.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 148.8)
		(end 144.4175 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 136.55)
		(end 178.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 116.55)
		(end 163.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 109.3)
		(end 161.1875 111.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 116.55)
		(end 168.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 148.8)
		(end 178.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 115.57)
		(end 170.6875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 146.55)
		(end 153.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 119.3)
		(end 158.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 119.3)
		(end 144.4175 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 138.8)
		(end 154.4175 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 115.57)
		(end 180.6875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 121.55)
		(end 161.1875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 111.55)
		(end 170.6875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 111.55)
		(end 161.1875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 116.55)
		(end 153.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 141.55)
		(end 150.6875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 139.3)
		(end 178.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 109.3)
		(end 148.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 129.3)
		(end 161.1875 131.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 111.55)
		(end 160.6875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 119.3)
		(end 151.1875 121.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 141.55)
		(end 178.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 126.55)
		(end 163.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 136.55)
		(end 158.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 115.57)
		(end 171.1875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 109.3)
		(end 164.4175 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 111.55)
		(end 150.6875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 116.55)
		(end 173.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 129.3)
		(end 178.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 138.8)
		(end 174.4175 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 145.57)
		(end 171.1875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 111.55)
		(end 151.1875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 128.8)
		(end 168.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 129.3)
		(end 148.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 121.55)
		(end 141.1875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 139.3)
		(end 171.1875 141.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 136.55)
		(end 153.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 139.3)
		(end 144.4175 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 145.57)
		(end 170.6875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 119.3)
		(end 141.1875 121.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 139.3)
		(end 154.4175 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 141.55)
		(end 171.1875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 118.8)
		(end 154.4175 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 131.55)
		(end 168.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 119.3)
		(end 178.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 129.3)
		(end 174.4175 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 131.55)
		(end 160.6875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 118.8)
		(end 164.4175 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 131.55)
		(end 148.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 140.184398 108.276898)
		(end 182.184398 150.276898)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 141.55)
		(end 161.1875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 118.8)
		(end 148.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 119.3)
		(end 168.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 141.55)
		(end 160.6875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 135.57)
		(end 171.1875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 111.55)
		(end 148.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 125.57)
		(end 180.6875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 146.55)
		(end 168.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 141.55)
		(end 158.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 111.55)
		(end 178.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 141.55)
		(end 180.6875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 115.57)
		(end 151.1875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 135.57)
		(end 150.6875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 148.8)
		(end 158.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.4575 128.8)
		(end 178.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 145.57)
		(end 160.6875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 125.57)
		(end 161.1875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 141.55)
		(end 168.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 131.55)
		(end 180.6875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 138.8)
		(end 158.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 146.55)
		(end 148.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 121.55)
		(end 171.1875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 125.57)
		(end 150.6875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 128.8)
		(end 154.4175 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 148.8)
		(end 164.4175 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 125.57)
		(end 151.1875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 139.3)
		(end 141.1875 141.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 119.3)
		(end 164.4175 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 116.55)
		(end 143.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 115.57)
		(end 160.6875 116.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 146.55)
		(end 158.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 126.55)
		(end 158.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 141.55)
		(end 141.1875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 135.57)
		(end 141.1875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 118.8)
		(end 158.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 126.55)
		(end 173.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 119.3)
		(end 161.1875 121.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 121.55)
		(end 180.6875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 131.55)
		(end 161.1875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 129.3)
		(end 144.4175 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 148.8)
		(end 154.4175 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 126.55)
		(end 148.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 111.55)
		(end 168.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 121.55)
		(end 151.1875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 109.3)
		(end 144.4175 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 129.3)
		(end 154.4175 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 141.55)
		(end 170.6875 142.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.4375 128.8)
		(end 164.4175 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 125.57)
		(end 141.1875 126.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 135.57)
		(end 180.6875 136.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 139.3)
		(end 174.4175 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 136.55)
		(end 148.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 121.55)
		(end 170.6875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 109.3)
		(end 174.4175 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 121.55)
		(end 150.6875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.1875 111.55)
		(end 171.1875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 145.57)
		(end 141.1875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 109.3)
		(end 151.1875 111.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 119.3)
		(end 174.4175 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 131.55)
		(end 151.1875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 116.55)
		(end 158.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.1875 126.55)
		(end 153.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 121.55)
		(end 178.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 121.55)
		(end 160.6875 122.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.4575 118.8)
		(end 168.4375 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 148.8)
		(end 148.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.4575 139.3)
		(end 148.4375 139.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.1875 131.55)
		(end 141.1875 132.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 109.3)
		(end 171.1875 111.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.6875 111.55)
		(end 180.6875 112.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.6875 111.55)
		(end 158.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 121.55)
		(end 168.4375 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 129.3)
		(end 151.1875 131.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 129.3)
		(end 158.4375 129.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 129.3)
		(end 171.1875 131.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 136.55)
		(end 163.4375 138.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4375 109.3)
		(end 141.1875 111.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 145.57)
		(end 161.1875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.4575 109.3)
		(end 158.4375 109.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4375 118.8)
		(end 174.4175 118.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.4375 119.3)
		(end 154.4175 119.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.6875 126.55)
		(end 168.4375 128.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.6875 145.57)
		(end 150.6875 146.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1875 146.55)
		(end 163.4375 148.8)
		(layer "Edge.Cuts")
	)
	(gr_text "tc"
		(at 170.5445 124.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 147.6675 126.41 45)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 172.1675 116.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 180.5445 124.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 145.2675 138.69 0)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 142.1675 146.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 162.1675 136.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 159.0175 137.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 165.2675 148.69 0)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 157.6675 126.41 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 156.8475 119.41 180)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 175.2675 118.69 0)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 156.8475 139.41 180)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 160.5445 124.364 90)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 159.0175 147.82 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 171.2975 113 -90)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 152.1675 116.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 149.6575 141.14 135)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 160.5445 114.364 90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 179.6575 111.14 135)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 149.0175 127.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 147.6675 136.41 45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 149.6575 131.14 135)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 161.2975 113 -90)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 176.8475 129.41 180)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 151.2975 123 -90)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 159.0175 117.82 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 156.8475 109.41 180)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 177.6675 136.41 45)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 170.5445 134.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 145.2675 128.69 0)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 151.2975 143 -90)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 172.1675 126.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 179.0175 147.82 45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 169.6575 131.14 135)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 165.2675 118.69 0)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 159.6575 141.14 135)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 177.6675 116.41 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 171.2975 123 -90)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 166.8475 109.41 180)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 162.1675 126.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 149.0175 117.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 175.2675 128.69 0)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 150.5445 114.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 165.2675 128.69 0)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 150.5445 144.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 157.6675 146.41 45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 169.6575 141.14 135)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 166.8475 129.41 180)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 151.2975 133 -90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 159.6575 121.14 135)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 150.5445 134.364 90)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 160.5445 144.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 157.6675 136.41 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 166.8475 139.41 180)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 172.1675 136.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 169.0175 137.82 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 161.2975 123 -90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 149.6575 121.14 135)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 162.1675 116.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 179.0175 127.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 155.2675 148.69 0)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 172.1675 146.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 167.6675 116.41 45)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 177.6675 126.41 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 141.2975 113 -90)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 165.2675 138.69 0)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 159.0175 127.82 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 146.8475 139.41 180)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 141.2975 133 -90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 169.6575 121.14 135)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 179.0175 117.82 45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 169.0175 117.82 45)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 180.5445 114.364 90)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 166.8475 119.41 180)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 167.6675 136.41 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 141.2975 123 -90)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 161.2975 133 -90)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 152.1675 146.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 176.8475 109.41 180)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 142.1675 116.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 152.1675 136.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 149.6575 111.14 135)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 162.1675 146.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 149.0175 137.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 167.6675 126.41 45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 175.2675 138.69 0)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 146.8475 129.41 180)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 169.6575 111.14 135)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 155.2675 118.69 0)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 180.5445 144.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 147.6675 116.41 45)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 177.6675 146.41 45)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 170.5445 114.364 90)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 147.6675 146.41 45)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 159.6575 131.14 135)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 159.6575 111.14 135)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 169.0175 127.82 45)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 152.1675 126.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 146.8475 119.41 180)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 179.0175 137.82 45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 161.2975 143 -90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 179.6575 121.14 135)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 179.6575 141.14 135)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 167.6675 146.41 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 156.8475 129.41 180)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 141.2975 143 -90)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 150.5445 124.364 90)
		(layer "F.SilkS")
	)
	(gr_text "gv"
		(at 179.6575 131.14 135)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 149.0175 147.82 45)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 170.5445 144.364 90)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 160.5445 134.364 90)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 171.2975 133 -90)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 146.8475 109.41 180)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 142.1675 136.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 171.2975 143 -90)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 176.8475 119.41 180)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 151.2975 113 -90)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 145.2675 148.69 0)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 145.2675 118.69 0)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 142.1675 126.98 -45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 155.2675 138.69 0)
		(layer "F.SilkS")
	)
	(gr_text "rs"
		(at 157.6675 116.41 45)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 176.8475 139.41 180)
		(layer "F.SilkS")
	)
	(gr_text "tc"
		(at 180.5445 134.364 90)
		(layer "F.SilkS")
	)
	(gr_text "3v"
		(at 169.0175 147.82 45)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 175.2675 148.69 0)
		(layer "F.SilkS")
	)
	(gr_text "rd"
		(at 155.2675 128.69 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 170.6875 109.3) (xy 170.6875 118.8) (xy 161.18262 118.81504) (xy 161.1875 109.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 160.6875 119.3) (xy 160.6875 128.8) (xy 151.18262 128.81504) (xy 151.1875 119.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 160.6875 139.3) (xy 160.6875 148.8) (xy 151.18262 148.81504) (xy 151.1875 139.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 160.6875 129.3) (xy 160.6875 138.8) (xy 151.18262 138.81504) (xy 151.1875 129.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 160.6875 109.3) (xy 160.6875 118.8) (xy 151.18262 118.81504) (xy 151.1875 109.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 150.6875 129.3) (xy 150.6875 138.8) (xy 141.18262 138.81504) (xy 141.1875 129.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 170.6875 139.3) (xy 170.6875 148.8) (xy 161.18262 148.81504) (xy 161.1875 139.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 150.6875 139.3) (xy 150.6875 148.8) (xy 141.18262 148.81504) (xy 141.1875 139.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 180.6875 119.3) (xy 180.6875 128.8) (xy 171.18262 128.81504) (xy 171.1875 119.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 180.6875 109.3) (xy 180.6875 118.8) (xy 171.18262 118.81504) (xy 171.1875 109.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 170.6875 119.3) (xy 170.6875 128.8) (xy 161.18262 128.81504) (xy 161.1875 119.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 150.6875 109.3) (xy 150.6875 118.8) (xy 141.18262 118.81504) (xy 141.1875 109.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 180.6875 139.3) (xy 180.6875 148.8) (xy 171.18262 148.81504) (xy 171.1875 139.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 180.6875 129.3) (xy 180.6875 138.8) (xy 171.18262 138.81504) (xy 171.1875 129.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 150.6875 119.3) (xy 150.6875 128.8) (xy 141.18262 128.81504) (xy 141.1875 119.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.15)
			(thermal_bridge_width 0.5)
			(hatch_thickness 1)
			(hatch_gap 1)
			(hatch_orientation 0)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 170.6875 129.3) (xy 170.6875 138.8) (xy 161.18262 138.81504) (xy 161.1875 129.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.6875 119.3) (xy 150.6875 128.8) (xy 141.18262 128.81504) (xy 141.1875 119.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.6875 109.3) (xy 150.6875 118.8) (xy 141.18262 118.81504) (xy 141.1875 109.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.6875 129.3) (xy 150.6875 138.8) (xy 141.18262 138.81504) (xy 141.1875 129.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.6875 139.3) (xy 160.6875 148.8) (xy 151.18262 148.81504) (xy 151.1875 139.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.6875 129.3) (xy 160.6875 138.8) (xy 151.18262 138.81504) (xy 151.1875 129.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.6875 119.3) (xy 170.6875 128.8) (xy 161.18262 128.81504) (xy 161.1875 119.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.6875 139.3) (xy 170.6875 148.8) (xy 161.18262 148.81504) (xy 161.1875 139.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.6875 139.3) (xy 180.6875 148.8) (xy 171.18262 148.81504) (xy 171.1875 139.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.6875 129.3) (xy 170.6875 138.8) (xy 161.18262 138.81504) (xy 161.1875 129.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.6875 129.3) (xy 180.6875 138.8) (xy 171.18262 138.81504) (xy 171.1875 129.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.6875 109.3) (xy 180.6875 118.8) (xy 171.18262 118.81504) (xy 171.1875 109.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.6875 139.3) (xy 150.6875 148.8) (xy 141.18262 148.81504) (xy 141.1875 139.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.6875 109.3) (xy 170.6875 118.8) (xy 161.18262 118.81504) (xy 161.1875 109.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.6875 119.3) (xy 180.6875 128.8) (xy 171.18262 128.81504) (xy 171.1875 119.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.6875 109.3) (xy 160.6875 118.8) (xy 151.18262 118.81504) (xy 151.1875 109.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.6875 119.3) (xy 160.6875 128.8) (xy 151.18262 128.81504) (xy 151.1875 119.3)
			)
		)
	)
)
